# Notch Filter

### From Audacity Development Manual

Notch Filter sharply attenuates frequency-specific noise like mains hum or electrical whistle with minimal damage to the remaining audio, by cutting a "notch" out of the frequency spectrum at that point.

  Accessed by: Effect > Notch Filter...

## Frequency

Enter any frequency up to half the sample rate into the frequency text box (default is 60 Hz). Frequency greater than half the sample rate of the track are not valid because a track can only contain frequencies up to half its sample rate.

## Q factor

This determines the width of the notch cut from your audio (default value is 1). Values above 1 create a narrower notch, and values below 1 create a wider notch. The Q Factor must be at least 0.1).

## The buttons

Clicking on the command buttons give the following results:

- Manage gives a dropdown menu enabling you to manage presets for the tool and to see some detail about the tool. For details see Manage presets.
- Preview plays a short preview of what the audio would sound like if the effect is applied with the current settings, without making actual changes to the audio. The length of preview is determined by your setting in Edit > Preferences > Playback, the default setting is 6 seconds.
- Debug applies the effect to the selected audio with the current effect settings, but unlike OK the effect runs in debug mode. This is primarily of use when writing or editing Nyquist plug-ins.
  - In addition to the normal plug-in behavior, a "debug window" opens to display error messages, normally the debug window will be empty.
- OK applies the effect to the selected audio with the current effect settings.
- Cancel aborts the effect and leaves the audio unchanged.

## Examples

### Example 1: Mains Hum Removal

Choose 60 Hz as "Frequency" for North America, or 50 Hz for the United Kingdom and most other countries. A table of mains frequencies by country is here.

Recorded hum often contains noisy harmonic frequencies above the fundamental frequency of the hum. A good approach is thus to apply Notch Filter to the fundamental hum frequency (for example, 50 Hz or 60 Hz), then use Analyze > Plot Spectrum... to identify other broad noise spikes (for example, at 180 Hz and 300 Hz). You may want to increase the spectrum Size and use the "Log" Axis to see more clearly. Run Notch Filter again at each of the other noise frequencies, then use Effect > Noise Reduction at mild settings to remove any residual harmonics.

- It is recommended to increase the Q factor when removing higher harmonics so as to lessen possible audio artifacts. Generally, a Q of between 2 and 10 works well for mains hum removal. Choosing appropriate Frequency and Q factor settings from the noise spikes in Plot Spectrum is an approximation, due to inevitable interpolation errors from whichever "windowing" function is chosen. However a good method for calculating Frequency and Q factor from Plot Spectrum can be found in this Audacity Forum topic.

The below image shows a spectrum plot of some music from which a notch of 60 Hz hum has been cut. Before applying the effect, the hum displayed a prominent spike at this frequency, extending to the top of the graph.

Depending on the audio, you might find in this case that the spectrum had been notched too deeply, thus affecting the content, and that a higher Q factor would have been preferred. You might want to notch the visible spikes at about 100 and 350 Hz as well. As always with Audacity, you can Edit > Undo and experiment with different notch filter settings.

### Example 2: High pitched whistle

In this case the frequency analysis at Analyze > Plot Spectrum... is fairly smooth except for a tall peak on the right. Place the mouse's cross-hair pointer over that peak. Audacity shows the peak more accurately to be at 18996 Hz which will be the frequency to enter in Notch Filter.

## Links

|< Index of Effects, Generators and Analyzers

|< Effect Menu

##### Views

##### Useful External Links

- Forum
- Wiki
- Latest Release