| Home
| Previous
| Next
| Up

GA_monitor

Declaration

typedef struct {
char mfr[MONITOR_MFR_LEN+1];
char model[MONITOR_MODEL_LEN+1];
char PNPID[8];
uchar maxResolution;
uchar minHScan;
uchar maxHScan;
uchar minVScan;
uchar maxVScan;
uchar flags;
} GA_monitor

Prototype In

snap/monitor.h

Description

Monitor configuration information structure. This structure defines the capabilities of the attached display monitor, and is used internally in SNAP Graphics to decide what features the driver should report for the attached monitor.

Members

mfr | Monitor manufacturer (key)
model | Monitor model name (sub-key)
PNPID | Plug and Play ID (optional)
maxResolution | Maximum resolution id
minHScan | Minimum horizontal scan
maxHScan | Maximum horizontal scan
minVScan | Minimum vertical scan
maxVScan | Maximum vertical scan
flags | Capabilities flags

Copyright © 2002 SciTech Software, Inc. Visit our web site at http://www.scitechsoft.com