| Home
| Previous
| Next
| Up

PCIAGPStatus

Declaration

typedef struct {
uint rate:4;
uint fastWrite:1;
uint fourGB:1;
uint rsvd1:3;
uint sideBandAddressing:1;
uint rsvd2:14;
uint requestQueueDepthMaximum:8;
} PCIAGPStatus

Prototype In

pcilib.h

Description

Structure defining the PCI AGP status register contents

Members

rate | Supported AGP rate (1-8x)
fastWrite | AGP FastWrite supported
fourGB | 4GB addressing supported
rsvd1 | Reserved; not used
sideBandAddressing | Side band addressing supported
rsvd2 | Reserved; not used
requestQueueDepthMaximum | Maximum request queue depth

Copyright © 2002 SciTech Software, Inc. Visit our web site at http://www.scitechsoft.com