| Home
| Previous
| Next
| Up

Set8BitDAC

Allow the RAMDAC width to be changed at runtime

Declaration

ibool GA_VBEFuncs::Set8BitDAC(
ibool enable)

Prototype In

snap/graphics.h

Return Value

True if request fulfilled, false if not

Description

This function allows the RAMDAC pixel width to be changed betwen 8-bit per primary mode or the VGA compatible 6-bit per primary mode. This primary use of this function is to allow emulation of VESA VBE/Core functions on top of native SNAP drivers (ie: DOS box support in Windows etc).

See Also

SetBytesPerLine, SetPaletteData, GetPaletteData

Copyright © 2002 SciTech Software, Inc. Visit our web site at http://www.scitechsoft.com