| Home
| Previous
| Next
| Up

### Software driven display start address swapping

If the hardware does not support a free running stereoscopic display mode, a timer driven, software driven stereoscopic display can be supported on some platforms. See the GA_softStereoInit function for information on how to set up software stereo support on supported platforms.

Copyright © 2002 SciTech Software, Inc. Visit our web site at http://www.scitechsoft.com