| Home
| Previous
| Next
| Up

EDID_flags

Declaration

typedef enum {
EDID_DPMSStandBy = 0x0001,
EDID_DPMSSuspend = 0x0002,
EDID_DPMSOff = 0x0004,
EDID_DPMSEnabled = 0x0007,
EDID_GTFEnabled = 0x0008,
EDID_DDC2AB = 0x0010,
EDID_Blank2Blank = 0x0020,
EDID_SyncSeparate = 0x0040,
EDID_SyncComposite = 0x0080,
EDID_SyncOnGreen = 0x0100,
EDID_NeedSerration = 0x0200,
EDID_PreferredTiming = 0x0400
} EDID_flags

Prototype In

snap/ddc.h

Description

This enumeration defines the values stored in the flags field of the EDID_record structure.

Members

EDID_DPMSStandBy | The DPMS Standby state is supported
EDID_DPMSSuspend | The DPMS Suspend state is supported
EDID_DPMSOff | The DPMS Off state is supported
EDID_DPMSEnabled | Monitor supports DPMS Power Management
EDID_GTFEnabled | Monitor supports GTF timings
EDID_DDC2AB | Monitor supports DDC2AB interface
EDID_Blank2Blank | Monitor requires Blank-to-Blank setup
EDID_SyncSeparate | Monitor supports separate syncs
EDID_SyncComposite | Monitor supports composite syncs
EDID_SyncOnGreen | Monitor supports Sync on Green
EDID_NeedSerration | VSync serration is required
EDID_PreferredTiming | Detailed timing 1 is preferred timing for monitor

Copyright © 2002 SciTech Software, Inc. Visit our web site at http://www.scitechsoft.com