DDC_ChannelsType

Declaration

typedef enum {
SCI_channelMonitorPrimary = 0x0000,
SCI_channelMonitorSecondary = 0x0001,
SCI_channelTVTuner = 0x0100
} DDC_ChannelsType

Prototype In

snap/ddc.h

Description

Flags passed to the Serial Control Interface functions to determine what I2C communications channel should be used. Usually the CRT monitor channel is used, but you can use different channels to control different devices.

Members

SCI_channelMonitorPrimary | Primary head display monitor channel
SCI_channelMonitorSecondary | Secondary head display monitor channel
SCI_channelTVTuner | TV-Tuner channel

Copyright © 2002 SciTech Software, Inc. Visit our web site at http://www.scitechsoft.com