| Home
| Previous
| Next
| Up

### Device Driver Control Functions

These functions are members of the GA_driverFuncs group. The functions form the main device driver functions that allow the application to change the display start address, program the color palette, program the gamma correction ramp and synchronize with the vertical refresh of the display.

EnableStereoMode | GetCurrentScanLine
GetDisplayStartStatus | GetGammaCorrectData
GetGammaCorrectDataExt | GetPaletteData
GetPaletteDataExt | GetVSyncWidth
IsVSync | SetBank
SetDisplayStart | SetDisplayStartXY
SetGammaCorrectData | SetGammaCorrectDataExt
SetPaletteData | SetPaletteDataExt
SetStereoDisplayStart | SetVSyncWidth
WaitVSync |

Copyright © 2002 SciTech Software, Inc. Visit our web site at http://www.scitechsoft.com