| Home
| Previous
| Next
| Up

GA_monitorFlagsType

Declaration

typedef enum {
Monitor_DPMSEnabled = 0x01,
Monitor_GTFEnabled = 0x02,
Monitor_FixedFreq = 0x04,
Monitor_HSyncNeg = 0x08,
Monitor_VSyncNeg = 0x10,
Monitor_16to9 = 0x20,
Monitor_Exclude4to3 = 0x40,
Monitor_Changed = 0x80
} GA_monitorFlagsType

Prototype In

snap/monitor.h

Description

This enumeration defines the flags for the capabilities for monitors as defined in the GA_monitor record.

Members

Monitor_DPMSEnabled | Monitor supports DPMS Power Management
Monitor_GTFEnabled | Monitor supports VESA Generalised Timing Formula
Monitor_FixedFreq | Monitor is a fixed frequency monitor
Monitor_HSyncNeg | HSync- is required for fixed frequency
Monitor_VSyncNeg | VSync- is required for fixed frequency
Monitor_16to9 | Monitor supports 16:9 aspect ratio modes
Monitor_Exclude4to3 | Driver should execlude all 4:3 aspect modes
Monitor_Changed | Monitor record has been changed

Copyright © 2002 SciTech Software, Inc. Visit our web site at http://www.scitechsoft.com