| Home
| Previous
| Next
| Up

WaitVSync

Waits until the graphics card enters the vertical retrace interval.

Declaration

void NAPI GA_driverFuncs::WaitVSync(void)

Prototype In

snap/graphics.h

Description

This function waits until the CRTC controller is enters the start of the vertical retrace interval and then returns.

See Also

IsVSync

Copyright © 2002 SciTech Software, Inc. Visit our web site at http://www.scitechsoft.com