GetCRTCTimings

Returns the current CRTC timings for the active display mode.

Declaration

void NAPI GA_initFuncs::GetCRTCTimings(
GA_CRTCInfo *crtc)

Prototype In

snap/graphics.h

Parameters

crtc | Place to store the active CRTC timings

Description

This function returns a copy of the currently active CRTC timings for the active display mode in the driver. This function is mostly used for interactive centering and refresh control in utility programs.

See Also

SetCRTCTimings, GetCurrentRefreshRate, SetGlobalRefresh, GA_saveCRTCTimings, GA_restoreCRTCTimings, GA_getCRTCTimings, GA_setCRTCTimings, GA_setDefaultRefresh

Copyright © 2002 SciTech Software, Inc. Visit our web site at http://www.scitechsoft.com