| Home
| Previous
| Next
| Up

MCS_begin

Checks to see if DDC/CI communication is available and opens it

Declaration

int NAPI MCS_begin(
GA_devCtx *dc)

Prototype In

snap/ddc.h

Parameters

dc | SNAP device driver to use for communications

Return Value

0 if DDC available, 1 if not available, -1 if unable to communicate via DDC

Description

Obsolete. Use MCS_beginExt instead.

See Also

MCS_beginExt

Copyright © 2002 SciTech Software, Inc. Visit our web site at http://www.scitechsoft.com