This is a stock boot0002.img with a 1.2.10 kernel
instead of 1.2.8.  It fixes some problems with the
TEAC CD-55A drive.  Note:  It does not have SCSI in
it.  If you require SCSI or an ethernet card to do your
install along with this drive, please email support@redhat.com.


