1210/boot0002.img:

This is the image to try for those of you with the TEAC CD-55A.  It
has no drivers in it other than the sbpcd driver, so you'll need 
to install with this and then build your own newer kernel for 
things like SCSI and network cards.

1210/boot0000.img:

This is a 1.2.10 boot image.  

mcdboot.img:

This is a boot disk compiled with only IDE and Mitsumi CD ROM
support with the interface hard coded to address 0x340 and 
interrupt 11.

1211/boot0011.img.gz

Stock boot0011 except it is version 1.2.11 instead of 1.2.8 that shipped
with the original mothers day release.

1211/booterik.img.gz

This was built for Erik Raymond, but in case anyone else needs this
config, it has Adaptec 1542 only, plus PPP, SLIP, CSLIP, PCI support,
and printer support.  No other drivers compiled in.

1211/boot0000.img.gz:

1.2.11 boot0000 image.  

1211/bootcomp.img:

actually a 1.2.0 boot image for Compaq XL-566 and similar models that
use the AM53C974 and AM79C974 SCSI chipsets.



--Donnie
