MGL_bitBlt

Blts a block of image data from one device context into another.

Declaration

void MGL_bitBlt(
MGLDC *dst,
MGLDC *src,
rect_t r,
int dstLeft,
int dstTop,
int op)

Prototype In

mgraph.h

Parameters

dst | Destination device context
src | Source device context
r | Rectangle defining are to Blt from
dstLeft | Left coordinate to Blt to
dstTop | Right coordinate to Blt to
op | Write mode to use during Blt

Description

This function is the same as MGL_bitBltCoord, however it takes entire rectangles as parameters instead of coordinates.

See Also

MGL_bitBlt, MGL_bitBltCoord, MGL_srcTransBlt, MGL_srcTransBltCoord, MGL_dstTransBlt, MGL_dstTransBltCoord, MGL_bitBltPatt, MGL_bitBltPattCoord, MGL_bitBltFx, MGL_bitBltFxCoord, MGL_stretchBlt, MGL_stretchBltCoord, MGL_stretchBltFx, MGL_stretchBltFxCoord, MGL_copyPage, MGL_copyPageCoord

Copyright © 2002 SciTech Software, Inc. Visit our web site at http://www.scitechsoft.com