| Home
| Previous
| Next
| Up

GA_OutputFlagsType

Declaration

typedef enum {
gaOUTPUT_CRT = 0x0001,
gaOUTPUT_LCD = 0x0002,
gaOUTPUT_DFP = 0x0400,
gaOUTPUT_TV = 0x0004,
gaOUTPUT_SELECTMASK = 0x0407,
gaOUTPUT_TVNTSC = 0x0008,
gaOUTPUT_TVNTSC_J = 0x0010,
gaOUTPUT_TVPAL = 0x0020,
gaOUTPUT_TVPAL_M = 0x0040,
gaOUTPUT_TVPAL_60 = 0x0080,
gaOUTPUT_TVPAL_CN = 0x0100,
gaOUTPUT_TVSCART_PAL = 0x0200,
gaOUTPUT_TVUNDERSCAN = 0x0000,
gaOUTPUT_TVOVERSCAN = 0x8000,
gaOUTPUT_TVCOLORMASK = 0x03F8
} GA_OutputFlagsType

Prototype In

snap/graphics.h

Description

Flags for the different output displays supported by the driver. These flags are passed to the SetDisplayOutput function to change the currently active display device and the GetDisplayDevice function to determine what devices are currenlty being used to display output.

Note: The color format for TV modes may be specified, or it may not. In the case where the color format is not specified, the currently active color format will be used. In some cases the color format is set in hardware and cannot be changed.

Members

gaOUTPUT_CRT | Indicates output is sent to CRT display
gaOUTPUT_LCD | Indicates output is sent to LCD panel
gaOUTPUT_DFP | Indicates output is sent to external DFP connector
gaOUTPUT_TV | Indicates output is sent to TV connector
gaOUTPUT_SELECTMASK | Mask to mask out just the output selection
gaOUTPUT_TVNTSC | Set TVOut connector color format to NTSC
gaOUTPUT_TVNTSC_J | Set TVOut connector color format to NTSC-J
gaOUTPUT_TVPAL | Set TVOut connector color format to PAL
gaOUTPUT_TVPAL_M | Set TVOut connector color format to PAL-M
gaOUTPUT_TVPAL_60 | Set TVOut connector color format to PAL-60
gaOUTPUT_TVPAL_CN | Set TVOut connector color format to PAL-CN
gaOUTPUT_TVSCART_PAL | Set TVOut connector color format to SCART-PAL
gaOUTPUT_TVUNDERSCAN | Indicates TV output should be underscanned
gaOUTPUT_TVOVERSCAN | Indicates TV output should be overscanned
gaOUTPUT_TVCOLORMASK | Mask to mask out TV color format

Copyright © 2002 SciTech Software, Inc. Visit our web site at http://www.scitechsoft.com