## RGB to 8/15/16 bit halftone dithering routines

The following functions allow you to obtain a copy of the SciTech MGL halftone palette, which is used for RGB to 8-bit real time dithering, and for performing the dither operation on a single pixel so you can implement your own real-time dithering routines. You can also do fast halftone dithering on 15-bit (5:5:5) and 16-bit (5:6:5) format pixels.

MGL_getHalfTonePalette | MGL_halfTonePixel
MGL_halfTonePixel555 | MGL_halfTonePixel565

Copyright © 2002 SciTech Software, Inc. Visit our web site at http://www.scitechsoft.com