| Home
| Previous
| Next
| Up

GA_modeFlagsType

Declaration

typedef enum {
gaDontClear = 0x8000,
gaLinearBuffer = 0x4000,
ga6BitDAC = 0x2000,
gaNoAccel = 0x1000,
gaRefreshCtrl = 0x0800,
gaWindowedMode = 0x0400,
gaPartialModeSet = 0x0200,
gaModeMask = 0x01FF
} GA_modeFlagsType

Prototype In

snap/graphics.h

Description

This enumeration defines the flags for combining with graphics mode numbers to be passed to the SetVideoMode function.

Members

gaDontClear | Don't clear display memory
gaLinearBuffer | Enable linear framebuffer mode
ga6BitDAC | Set the mode with a 6-bit RAMDAC instead of 8
gaNoAccel | Set the mode without any acceleration support
gaRefreshCtrl | Enable refresh rate control
gaWindowedMode | Initialise for use in the current desktop mode
gaPartialModeSet | Initialise the driver internals, but don't program hardware
gaModeMask | Mask to remove flags and extract VBE mode number

Copyright © 2002 SciTech Software, Inc. Visit our web site at http://www.scitechsoft.com