GA_saveCRTCTimings

Save the CRTC timings to disk for the specified driver

Declaration

ibool NAPI GA_saveCRTCTimings(
GA_devCtx *dc)

Prototype In

snap/graphics.h

Parameters

dc | Device context to save CRTC timings information for

Return Value

True on success, false on error.

Description

This function saves the driver CRTC timings information to disk. If any of the timings for the driver have been changed via the SetCRTCTimings or SetGlobalRefresh functions, this will save those timings to disk to be used as the defaults from then on.

See Also

GA_restoreCRTCTimings, GetCRTCTimings, SaveCRTCTimings, SetGlobalRefresh, GA_saveModeProfile, GA_saveOptions

Copyright © 2002 SciTech Software, Inc. Visit our web site at http://www.scitechsoft.com