GetPaletteData

Returns the current hardware color palette in VBE/Core compatible mode

Declaration

void GA_VBEFuncs::GetPaletteData(
GA_palette *pal,
N_int32 num,
N_int32 index)

Prototype In

snap/graphics.h

Parameters

pal | Place to return the palette data
num | Number of palette entries to read
index | Index of first entry to read

Description

This function is similar to GetPaletteData, however the palette data is always read verbatim, and no palette translation occurs. Hence these functions are compatible with the way the VESA VBE/Core palette functions work, which is different to the native SNAP way of handling palette programming.

See Also

SetBytesPerLine, Set8BitDAC, SetPaletteData

Copyright © 2002 SciTech Software, Inc. Visit our web site at http://www.scitechsoft.com