| Home
| Previous
| Next
| Up

PM_setRealTimeClockFrequency

Set the real time clock frequency (for stereo modes).

Declaration

void PMAPI PM_setRealTimeClockFrequency(
int frequency)

Prototype In

pmapi.h

Parameters

frequency | New frequency to program the RTC to run at

Description

This function is used to change the real time clock frequency that is used for software stereo modes by the SNAP Graphics drivers. The interrupt handler must first be installed with the PM_setRealTimeClockHandler function.

See Also

PM_setRealTimeClockHandler, PM_stopRealTimeClock, PM_restartRealTimeClock, PM_restoreRealTimeClockHandler

Copyright © 2002 SciTech Software, Inc. Visit our web site at http://www.scitechsoft.com