| Home
| Previous
| Next
| Up

DDC_DPMSStatesType

Declaration

typedef enum {
DPMS_on = 0,
DPMS_standby = 1,
DPMS_suspend = 2,
DPMS_off = 4
} DDC_DPMSStatesType

Prototype In

snap/ddc.h

Description

DPMS state values to pass to the DPMSsetState device driver call. This enumeration defines the values to set a specific power down state, and are based on the values defined in the VESA DPMS 1.0 specification. Please consult this or later versions of this specification for more information.

Members

DPMS_on | Return the controller to the ON state
DPMS_standby | Set the controller to the Stand-By power down state
DPMS_suspend | Set the controller to the Suspend power down state
DPMS_off | Set the controller to the Off power down state

Copyright © 2002 SciTech Software, Inc. Visit our web site at http://www.scitechsoft.com